#### G.5.16 TMS320C6x Features ¶

The ‘`org.gnu.gdb.tic6x.core`’ feature is required for TMS320C6x targets. It should contain registers ‘`A0`’ through ‘`A15`’, registers ‘`B0`’ through ‘`B15`’, ‘`CSR`’ and ‘`PC`’.

The ‘`org.gnu.gdb.tic6x.gp`’ feature is optional. It should contain registers ‘`A16`’ through ‘`A31`’ and ‘`B16`’ through ‘`B31`’.

The ‘`org.gnu.gdb.tic6x.c6xp`’ feature is optional. It should contain registers ‘`TSR`’, ‘`ILC`’ and ‘`RILC`’.