Next: “Cannot insert breakpoints”, Previous: How to save breakpoints to a file, Up: Breakpoints, Watchpoints, and Catchpoints [Contents][Index]

#### 5.1.10 Static Probe Points

GDB supports SDT probes in the code. SDT stands for Statically Defined Tracing, and the probes are designed to have a tiny runtime code and data footprint, and no dynamic relocations.

Currently, the following types of probes are supported on ELF-compatible systems:

- `SystemTap` (http://sourceware.org/systemtap/) SDT probes5. `SystemTap` probes are usable from assembly, C and C`++` languages6.
- `DTrace` (http://oss.oracle.com/projects/DTrace) USDT probes. `DTrace` probes are usable from C and C`++` languages.

Some `SystemTap` probes have an associated semaphore variable; for instance, this happens automatically if you defined your probe using a DTrace-style `.d` file. If your probe has a semaphore, GDB will automatically enable it when you specify a breakpoint using the ‘`-probe-stap`’ notation. But, if you put a breakpoint at a probe’s location by some other method (e.g., `break file:line`), then GDB will not automatically set the semaphore. `DTrace` probes do not support semaphores.

You can examine the available static static probes using `info probes`, with optional arguments:

`info probes [type] [provider [name [objfile]]]`

  If given, type is either `stap` for listing `SystemTap` probes or `dtrace` for listing `DTrace` probes. If omitted all probes are listed regardless of their types.

  If given, provider is a regular expression used to match against provider names when selecting which probes to list. If omitted, probes by all probes from all providers are listed.

  If given, name is a regular expression to match against probe names when selecting which probes to list. If omitted, probe names are not considered when deciding whether to display them.

  If given, objfile is a regular expression used to select which object files (executable or shared libraries) to examine. If not given, all object files are considered.

`info probes all`

  List the available static probes, from all types.

Some probe points can be enabled and/or disabled. The effect of enabling or disabling a probe depends on the type of probe being handled. Some `DTrace` probes can be enabled or disabled, but `SystemTap` probes cannot be disabled.

You can enable (or disable) one or more probes using the following commands, with optional arguments:

`enable probes [provider [name [objfile]]]`

  If given, provider is a regular expression used to match against provider names when selecting which probes to enable. If omitted, all probes from all providers are enabled.

  If given, name is a regular expression to match against probe names when selecting which probes to enable. If omitted, probe names are not considered when deciding whether to enable them.

  If given, objfile is a regular expression used to select which object files (executable or shared libraries) to examine. If not given, all object files are considered.

`disable probes [provider [name [objfile]]]`

  See the `enable probes` command above for a description of the optional arguments accepted by this command.

A probe may specify up to twelve arguments. These are available at the point at which the probe is defined—that is, when the current PC is at the probe’s location. The arguments are available using the convenience variables (see Convenience Variables) `$_probe_arg0`…`$_probe_arg11`. In `SystemTap` probes each probe argument is an integer of the appropriate size; types are not preserved. In `DTrace` probes types are preserved provided that they are recognized as such by GDB; otherwise the value of the probe argument will be a long integer. The convenience variable `$_probe_argc` holds the number of arguments at the current probe point.

These variables are always available, but attempts to access them at any location other than a probe point will cause GDB to give an error message.

#### Footnotes

##### (5)

See http://sourceware.org/systemtap/wiki/AddingUserSpaceProbingToApps for more information on how to add `SystemTap` SDT probes in your applications.

##### (6)

See http://sourceware.org/systemtap/wiki/UserSpaceProbeImplementation for a good reference on how the SDT probes are implemented.

Next: “Cannot insert breakpoints”, Previous: How to save breakpoints to a file, Up: Breakpoints, Watchpoints, and Catchpoints [Contents][Index]