Next: Alpha, Previous: AArch64, Up: Architectures [Contents][Index]

#### 21.4.2 x86

`set struct-convention mode` ¶

  Set the convention used by the inferior to return `struct`s and `union`s from functions to mode. Possible values of mode are `"pcc"`, `"reg"`, and `"default"` (the default). `"default"` or `"pcc"` means that `struct`s are returned on the stack, while `"reg"` means that a `struct` or a `union` whose size is 1, 2, 4, or 8 bytes will be returned in a register.

`show struct-convention` ¶

  Show the current setting of the convention to return `struct`s from functions.

#### 21.4.2.1 Intel Memory Protection Extensions (MPX).

Memory Protection Extension (MPX) adds the bound registers ‘`BND0`’ 17 through ‘`BND3`’. Bound registers store a pair of 64-bit values which are the lower bound and upper bound. Bounds are effective addresses or memory locations. The upper bounds are architecturally represented in 1’s complement form. A bound having lower bound = 0, and upper bound = 0 (1’s complement of all bits set) will allow access to the entire address space.

‘`BND0`’ through ‘`BND3`’ are represented in GDB as ‘`bnd0raw`’ through ‘`bnd3raw`’. Pseudo registers ‘`bnd0`’ through ‘`bnd3`’ display the upper bound performing the complement of one operation on the upper bound value, i.e. when upper bound in ‘`bnd0raw`’ is 0 in the GDB ‘`bnd0`’ it will be `0xfff…`. In this sense it can also be noted that the upper bounds are inclusive.

As an example, assume that the register BND0 holds bounds for a pointer having access allowed for the range between 0x32 and 0x71. The values present on bnd0raw and bnd registers are presented as follows:

    	bnd0raw = {0x32, 0xffffffff8e}
    	bnd0 = {lbound = 0x32, ubound = 0x71} : size 64

This way the raw value can be accessed via bnd0raw…bnd3raw. Any change on bnd0…bnd3 or bnd0raw…bnd3raw is reflect on its counterpart. When the bnd0…bnd3 registers are displayed via Python, the display includes the memory size, in bits, accessible to the pointer.

Bounds can also be stored in bounds tables, which are stored in application memory. These tables store bounds for pointers by specifying the bounds pointer’s value along with its bounds. Evaluating and changing bounds located in bound tables is therefore interesting while investigating bugs on MPX context. GDB provides commands for this purpose:

`show mpx bound pointer` ¶

  Display bounds of the given pointer.

`set mpx bound pointer, lbound, ubound` ¶

  Set the bounds of a pointer in the bound table. This command takes three parameters: pointer is the pointers whose bounds are to be changed, lbound and ubound are new values for lower and upper bounds respectively.

Both commands are deprecated and will be removed in future versions of GDB. MPX itself was listed as removed by Intel in 2019.

When you call an inferior function on an Intel MPX enabled program, GDB sets the inferior’s bound registers to the init (disabled) state before calling the function. As a consequence, bounds checks for the pointer arguments passed to the function will always pass.

This is necessary because when you call an inferior function, the program is usually in the middle of the execution of other function. Since at that point bound registers are in an arbitrary state, not clearing them would lead to random bound violations in the called function.

You can still examine the influence of the bound registers on the execution of the called function by stopping the execution of the called function at its prologue, setting bound registers, and continuing the execution. For example:

    	$ break *upper
    	Breakpoint 2 at 0x4009de: file i386-mpx-call.c, line 47.
    	$ print upper (a, b, c, d, 1)
    	Breakpoint 2, upper (a=0x0, b=0x6e0000005b, c=0x0, d=0x0, len=48)....
    	$ print $bnd0
    	{lbound = 0x0, ubound = ffffffff} : size -1

At this last step the value of bnd0 can be changed for investigation of bound violations caused along the execution of the call. In order to know how to set the bound registers or bound table for the call consult the ABI.

#### 21.4.2.2 x87 registers

GDB provides access to the x87 state through the following registers:

- `$st0` to `st7`: `ST(0)` to `ST(7)` floating-point registers
- `$fctrl`: control word register (`FCW`)
- `$fstat`: status word register (`FSW`)
- `$ftag`: tag word (`FTW`)
- `$fiseg`: last instruction pointer segment
- `$fioff`: last instruction pointer
- `$foseg`: last data pointer segment
- `$fooff`: last data pointer
- `$fop`: last opcode

#### Footnotes

##### (17)

The register named with capital letters represent the architecture registers.

Next: Alpha, Previous: AArch64, Up: Architectures [Contents][Index]