Next: Stop Reply Packets, Previous: Standard Replies, Up: GDB Remote Serial Protocol [Contents][Index]

### E.3 Packets

The following table provides a complete list of all currently defined commands and their corresponding response data. See File-I/O Remote Protocol Extension, for details about the File I/O extension of the remote protocol.

Each packet’s description has a template showing the packet’s overall syntax, followed by an explanation of the packet’s meaning. We include spaces in some of the templates for clarity; these are not part of the packet’s syntax. No GDB packet uses spaces to separate its components. For example, a template like ‘`foo bar baz`’ describes a packet beginning with the three ASCII bytes ‘`foo`’, followed by a bar, followed directly by a baz. GDB does not transmit a space character between the ‘`foo`’ and the bar, or between the bar and the baz.

Several packets and replies include a thread-id field to identify a thread. Normally these are positive numbers with a target-specific interpretation, formatted as big-endian hex strings. A thread-id can also be a literal ‘`-1`’ to indicate all threads, or ‘`0`’ to pick any thread.

In addition, the remote protocol supports a multiprocess feature in which the thread-id syntax is extended to optionally include both process and thread ID fields, as ‘`ppid.tid`’. The pid (process) and tid (thread) components each have the format described above: a positive number with target-specific interpretation formatted as a big-endian hex string, literal ‘`-1`’ to indicate all processes or threads (respectively), or ‘`0`’ to indicate an arbitrary process or thread. Specifying just a process, as ‘`ppid`’, is equivalent to ‘`ppid.-1`’. It is an error to specify all processes but a specific thread, such as ‘`p-1.tid`’. Note that the ‘`p`’ prefix is not used for those packets and replies explicitly documented to include a process ID, rather than a thread-id.

The multiprocess thread-id syntax extensions are only used if both GDB and the stub report support for the ‘`multiprocess`’ feature using ‘`qSupported`’. See multiprocess extensions, for more information.

Note that all packet forms beginning with an upper- or lower-case letter, other than those described here, are reserved for future use.

Here are the packet descriptions.

‘`!`’ ¶

  Enable extended mode. In extended mode, the remote server is made persistent. The ‘`R`’ packet is used to restart the program being debugged.

  Reply:

  ‘`OK`’

    The remote target both supports and has enabled extended mode.

‘`?`’ ¶

  This is sent when connection is first established to query the reason the target halted. The reply is the same as for step and continue. This packet has a special interpretation when the target is in non-stop mode; see Remote Protocol Support for Non-Stop Mode.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`A arglen,argnum,arg,…`’ ¶

  Initialized `argv[]` array passed into program. arglen specifies the number of bytes in the hex encoded byte stream arg. See `gdbserver` for more details.

  Reply:

  ‘`OK`’

    The arguments were set.

‘`b baud`’ ¶

  (Don’t use this packet; its behavior is not well-defined.) Change the serial line speed to baud.

  JTC: When does the transport layer state change? When it’s received, or after the ACK is transmitted. In either case, there are problems if the command or the acknowledgment packet is dropped.

  Stan: If people really wanted to add something like this, and get it working for the first time, they ought to modify ser-unix.c to send some kind of out-of-band message to a specially-setup stub and have the switch happen "in between" packets, so that from remote protocol’s point of view, nothing actually happened.

‘`B addr,mode`’ ¶

  Set (mode is ‘`S`’) or clear (mode is ‘`C`’) a breakpoint at addr.

  Don’t use this packet. Use the ‘`Z`’ and ‘`z`’ packets instead (see insert breakpoint or watchpoint packet).

‘`bc`’

  Backward continue. Execute the target system in reverse. No parameter. See Running programs backward, for more information.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`bs`’

  Backward single step. Execute one instruction in reverse. No parameter. See Running programs backward, for more information.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`c [addr]`’ ¶

  Continue at addr, which is the address to resume. If addr is omitted, resume at current address.

  This packet is deprecated for multi-threading support. See vCont packet.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`C sig[;addr]`’ ¶

  Continue with signal sig (hex signal number). If ‘`;addr`’ is omitted, resume at same address.

  This packet is deprecated for multi-threading support. See vCont packet.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`d`’ ¶

  Toggle debug flag.

  Don’t use this packet; instead, define a general set packet (see General Query Packets).

‘`D`’ ¶
‘`D;pid`’

  The first form of the packet is used to detach GDB from the remote system. It is sent to the remote target before GDB disconnects via the `detach` command.

  The second form, including a process ID, is used when multiprocess protocol extensions are enabled (see multiprocess extensions), to detach only a specific process. The pid is specified as a big-endian hex string.

  Reply:

  ‘`OK`’

    for success

‘`F RC,EE,CF;XX`’ ¶

  A reply from GDB to an ‘`F`’ packet sent by the target. This is part of the File-I/O protocol extension. See File-I/O Remote Protocol Extension, for the specification.

‘`g`’

  Read general registers.

  Reply:

  ‘`XX…`’

    Each byte of register data is described by two hex digits. The bytes with the register are transmitted in target byte order. The size of each register and their position within the ‘`g`’ packet are determined by the target description (see Target Descriptions); in the absence of a target description, this is done using code internal to GDB; typically this is some customary register layout for the architecture in question.

    When reading registers, the stub may also return a string of literal ‘`x`’’s in place of the register data digits, to indicate that the corresponding register’s value is unavailable. For example, when reading registers from a trace frame (see Using the Collected Data), this means that the register has not been collected in the trace frame. When reading registers from a live program, this indicates that the stub has no means to access the register contents, even though the corresponding register is known to exist. Note that if a register truly does not exist on the target, then it is better to not include it in the target description in the first place.

    For example, for an architecture with 4 registers of 4 bytes each, the following reply indicates to GDB that registers 0 and 2 are unavailable, while registers 1 and 3 are available, and both have zero value:

        -> g
        <- xxxxxxxx00000000xxxxxxxx00000000

‘`G XX…`’ ¶

  Write general registers. See read registers packet, for a description of the XX… data.

  Reply:

  ‘`OK`’

    for success

‘`H op thread-id`’ ¶

  Set thread for subsequent operations (‘`m`’, ‘`M`’, ‘`g`’, ‘`G`’, et.al.). Depending on the operation to be performed, op should be ‘`c`’ for step and continue operations (note that this is deprecated, supporting the ‘`vCont`’ command is a better option), and ‘`g`’ for other operations. The thread designator thread-id has the format and interpretation described in thread-id syntax.

  Reply:

  ‘`OK`’

    for success

‘`i [addr[,nnn]]`’

  Step the remote target by a single clock cycle. If ‘`,nnn`’ is present, cycle step nnn cycles. If addr is present, cycle step starting at that address.

‘`I`’ ¶

  Signal, then cycle step. See step with signal packet. See cycle step packet.

‘`k`’ ¶

  Kill request.

  The exact effect of this packet is not specified.

  For a bare-metal target, it may power cycle or reset the target system. For that reason, the ‘`k`’ packet has no reply.

  For a single-process target, it may kill that process if possible.

  A multiple-process target may choose to kill just one process, or all that are under GDB’s control. For more precise control, use the vKill packet (see vKill packet).

  If the target system immediately closes the connection in response to ‘`k`’, GDB does not consider the lack of packet acknowledgment to be an error, and assumes the kill was successful.

  If connected using `target extended-remote`, and the target does not close the connection in response to a kill request, GDB probes the target state as if a new connection was opened (see ? packet).

‘`m addr,length`’ ¶

  Read length addressable memory units starting at address addr (see addressable memory unit). Note that addr may not be aligned to any particular boundary.

  The stub need not use any particular size or alignment when gathering data from memory for the response; even if addr is word-aligned and length is a multiple of the word size, the stub is free to use byte accesses, or not. For this reason, this packet may not be suitable for accessing memory-mapped I/O devices.

  Reply:

  ‘`XX…`’

    Memory contents; each byte is transmitted as a two-digit hexadecimal number. The reply may contain fewer addressable memory units than requested if the server was able to read only part of the region of memory.

  Unlike most packets, this packet does not support ‘`E.errtext`’-style textual error replies (see textual error reply).

‘`M addr,length:XX…`’ ¶

  Write length addressable memory units starting at address addr (see addressable memory unit). The data is given by XX…; each byte is transmitted as a two-digit hexadecimal number.

  Reply:

  ‘`OK`’

    All the data was written successfully. (If only part of the data was written, this command returns an error.)

‘`p n`’ ¶

  Read the value of register n; n is in hex. See read registers packet, for a description of how the returned register value is encoded.

  Reply:

  ‘`XX…`’

    the register’s value

‘`P n…=r…`’

  Write register n… with value r…. The register number n is in hexadecimal, and r… contains two hex digits for each byte in the register (target byte order).

  Reply:

  ‘`OK`’

    for success

‘`q name params…`’ ¶
‘`Q name params…`’

  General query (‘`q`’) and set (‘`Q`’). These packets are described fully in General Query Packets.

‘`r`’ ¶

  Reset the entire system.

  Don’t use this packet; use the ‘`R`’ packet instead.

‘`R XX`’ ¶

  Restart the program being debugged. The XX, while needed, is ignored. This packet is only available in extended mode (see extended mode).

  The ‘`R`’ packet has no reply.

‘`s [addr]`’ ¶

  Single step, resuming at addr. If addr is omitted, resume at same address.

  This packet is deprecated for multi-threading support. See vCont packet.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`S sig[;addr]`’

  Step with signal. This is analogous to the ‘`C`’ packet, but requests a single-step, rather than a normal resumption of execution.

  This packet is deprecated for multi-threading support. See vCont packet.

  Reply: See Stop Reply Packets, for the reply specifications.

‘`t addr:PP,MM`’ ¶

  Search backwards starting at address addr for a match with pattern PP and mask MM, both of which are are 4 byte long. There must be at least 3 digits in addr.

‘`T thread-id`’ ¶

  Find out if the thread thread-id is alive. See thread-id syntax.

  Reply:

  ‘`OK`’

    thread is still alive

‘`v`’

  Packets starting with ‘`v`’ are identified by a multi-letter name, up to the first ‘`;`’ or ‘`?`’ (or the end of the packet).

‘`vAttach;pid`’ ¶

  Attach to a new process with the specified process ID pid. The process ID is a hexadecimal integer identifying the process. In all-stop mode, all threads in the attached process are stopped; in non-stop mode, it may be attached without being stopped if that is supported by the target.

  This packet is only available in extended mode (see extended mode).

  Reply:

  ‘`Any stop packet`’

    for success in all-stop mode (see Stop Reply Packets)

  ‘`OK`’

    for success in non-stop mode (see Remote Protocol Support for Non-Stop Mode)

‘`vCont[;action[:thread-id]]…`’ ¶

  Resume the inferior, specifying different actions for each thread.

  For each inferior thread, the leftmost action with a matching thread-id is applied. Threads that don’t match any action remain in their current state. Thread IDs are specified using the syntax described in thread-id syntax. If multiprocess extensions (see multiprocess extensions) are supported, actions can be specified to match all threads in a process by using the ‘`ppid.-1`’ form of the thread-id. An action with no thread-id matches all threads. Specifying no actions is an error.

  Currently supported actions are:

  ‘`c`’

    Continue.

  ‘`C sig`’

    Continue with signal sig. The signal sig should be two hex digits.

  ‘`s`’

    Step.

  ‘`S sig`’

    Step with signal sig. The signal sig should be two hex digits.

  ‘`t`’

    Stop.

  ‘`r start,end`’

    Step once, and then keep stepping as long as the thread stops at addresses between start (inclusive) and end (exclusive). The remote stub reports a stop reply when either the thread goes out of the range or is stopped due to an unrelated reason, such as hitting a breakpoint. See range stepping.

    If the range is empty (start == end), then the action becomes equivalent to the ‘`s`’ action. In other words, single-step once, and report the stop (even if the stepped instruction jumps to start).

    (A stop reply may be sent at any point even if the PC is still within the stepping range; for example, it is valid to implement this packet in a degenerate way as a single instruction step operation.)

  The optional argument addr normally associated with the ‘`c`’, ‘`C`’, ‘`s`’, and ‘`S`’ packets is not supported in ‘`vCont`’.

  The ‘`t`’ action is only relevant in non-stop mode (see Remote Protocol Support for Non-Stop Mode) and may be ignored by the stub otherwise. A stop reply should be generated for any affected thread not already stopped. When a thread is stopped by means of a ‘`t`’ action, the corresponding stop reply should indicate that the thread has stopped with signal ‘`0`’, regardless of whether the target uses some other signal as an implementation detail.

  The server must ignore ‘`c`’, ‘`C`’, ‘`s`’, ‘`S`’, and ‘`r`’ actions for threads that are already running. Conversely, the server must ignore ‘`t`’ actions for threads that are already stopped.

  Note: In non-stop mode, a thread is considered running until GDB acknowledges an asynchronous stop notification for it with the ‘`vStopped`’ packet (see Remote Protocol Support for Non-Stop Mode).

  The stub must support ‘`vCont`’ if it reports support for multiprocess extensions (see multiprocess extensions).

  Reply: See Stop Reply Packets, for the reply specifications.

‘`vCont?`’ ¶

  Request a list of actions supported by the ‘`vCont`’ packet.

  Reply:

  ‘`vCont[;action…]`’

    The ‘`vCont`’ packet is supported. Each action is a supported command in the ‘`vCont`’ packet.

‘`vCtrlC`’ ¶

  Interrupt remote target as if a control-C was pressed on the remote terminal. This is the equivalent to reacting to the `^C` (‘`\003`’, the control-C character) character in all-stop mode while the target is running, except this works in non-stop mode. See interrupting remote targets, for more info on the all-stop variant.

  Reply:

  ‘`OK`’

    for success

‘`vFile:operation:parameter…`’ ¶

  Perform a file operation on the target system. For details, see Host I/O Packets.

‘`vFlashErase:addr,length`’ ¶

  Direct the stub to erase length bytes of flash starting at addr. The region may enclose any number of flash blocks, but its start and end must fall on block boundaries, as indicated by the flash block size appearing in the memory map (see Memory Map Format). GDB groups flash memory programming operations together, and sends a ‘`vFlashDone`’ request after each group; the stub is allowed to delay erase operation until the ‘`vFlashDone`’ packet is received.

  Reply:

  ‘`OK`’

    for success

‘`vFlashWrite:addr:XX…`’ ¶

  Direct the stub to write data to flash address addr. The data is passed in binary form using the same encoding as for the ‘`X`’ packet (see Binary Data). The memory ranges specified by ‘`vFlashWrite`’ packets preceding a ‘`vFlashDone`’ packet must not overlap, and must appear in order of increasing addresses (although ‘`vFlashErase`’ packets for higher addresses may already have been received; the ordering is guaranteed only between ‘`vFlashWrite`’ packets). If a packet writes to an address that was neither erased by a preceding ‘`vFlashErase`’ packet nor by some other target-specific method, the results are unpredictable.

  Reply:

  ‘`OK`’

    for success

  ‘`E.memtype`’

    for vFlashWrite addressing non-flash memory

‘`vFlashDone`’ ¶

  Indicate to the stub that flash programming operation is finished. The stub is permitted to delay or batch the effects of a group of ‘`vFlashErase`’ and ‘`vFlashWrite`’ packets until a ‘`vFlashDone`’ packet is received. The contents of the affected regions of flash memory are unpredictable until the ‘`vFlashDone`’ request is completed.

‘`vKill;pid`’ ¶

  Kill the process with the specified process ID pid, which is a hexadecimal integer identifying the process. This packet is used in preference to ‘`k`’ when multiprocess protocol extensions are supported; see multiprocess extensions.

  Reply:

  ‘`OK`’

    for success

‘`vMustReplyEmpty`’ ¶

  The correct reply to an unknown ‘`v`’ packet is to return the empty string, however, some older versions of `gdbserver` would incorrectly return ‘`OK`’ for unknown ‘`v`’ packets.

  The ‘`vMustReplyEmpty`’ is used as a feature test to check how `gdbserver` handles unknown packets, it is important that this packet be handled in the same way as other unknown ‘`v`’ packets. If this packet is handled differently to other unknown ‘`v`’ packets then it is possible that GDB may run into problems in other areas, specifically around use of ‘`vFile:setfs:`’.

‘`vRun;filename[;argument]…`’ ¶

  Run the program filename, passing it each argument on its command line. The file and arguments are hex-encoded strings. If filename is an empty string, the stub may use a default program (e.g. the last program run). The program is created in the stopped state.

  This packet is only available in extended mode (see extended mode).

  Reply:

  ‘`Any stop packet`’

    for success (see Stop Reply Packets)

‘`vStopped`’ ¶

  See Notification Packets.

‘`X addr,length:XX…`’

  Write data to memory, where the data is transmitted in binary. Memory is specified by its address addr and number of addressable memory units length (see addressable memory unit); ‘`XX…`’ is binary data (see Binary Data).

  Reply:

  ‘`OK`’

    for success

‘`z type,addr,kind`’
‘`Z type,addr,kind`’

  Insert (‘`Z`’) or remove (‘`z`’) a type breakpoint or watchpoint starting at address address of kind kind.

  Each breakpoint and watchpoint packet type is documented separately.

  Implementation notes: A remote target shall return an empty string for an unrecognized breakpoint or watchpoint packet type. A remote target shall support either both or neither of a given ‘`Ztype…`’ and ‘`ztype…`’ packet pair. To avoid potential problems with duplicate packets, the operations should be implemented in an idempotent way.

‘`z0,addr,kind`’ ¶
‘`Z0,addr,kind[;cond_list…][;cmds:persist,cmd_list…]`’

  Insert (‘`Z0`’) or remove (‘`z0`’) a software breakpoint at address addr of type kind.

  A software breakpoint is implemented by replacing the instruction at addr with a software breakpoint or trap instruction. The kind is target-specific and typically indicates the size of the breakpoint in bytes that should be inserted. E.g., the ARM and MIPS can insert either a 2 or 4 byte breakpoint. Some architectures have additional meanings for kind (see Architecture-Specific Protocol Details); if no architecture-specific value is being used, it should be ‘`0`’. kind is hex-encoded. cond_list is an optional list of conditional expressions in bytecode form that should be evaluated on the target’s side. These are the conditions that should be taken into consideration when deciding if the breakpoint trigger should be reported back to GDB.

  See also the ‘`swbreak`’ stop reason (see swbreak stop reason) for how to best report a software breakpoint event to GDB.

  The cond_list parameter is comprised of a series of expressions, concatenated without separators. Each expression has the following form:

  ‘`X len,expr`’

    len is the length of the bytecode expression and expr is the actual conditional expression in bytecode form.

  The optional cmd_list parameter introduces commands that may be run on the target, rather than being reported back to GDB. The parameter starts with a numeric flag persist; if the flag is nonzero, then the breakpoint may remain active and the commands continue to be run even when GDB disconnects from the target. Following this flag is a series of expressions concatenated with no separators. Each expression has the following form:

  ‘`X len,expr`’

    len is the length of the bytecode expression and expr is the actual commands expression in bytecode form.

  Implementation note: It is possible for a target to copy or move code that contains software breakpoints (e.g., when implementing overlays). The behavior of this packet, in the presence of such a target, is not defined.

  Reply:

  ‘`OK`’

    success

‘`z1,addr,kind`’ ¶
‘`Z1,addr,kind[;cond_list…][;cmds:persist,cmd_list…]`’

  Insert (‘`Z1`’) or remove (‘`z1`’) a hardware breakpoint at address addr.

  A hardware breakpoint is implemented using a mechanism that is not dependent on being able to modify the target’s memory. The kind, cond_list, and cmd_list arguments have the same meaning as in ‘`Z0`’ packets.

  Implementation note: A hardware breakpoint is not affected by code movement.

  Reply:

  ‘`OK`’

    success

‘`z2,addr,kind`’ ¶
‘`Z2,addr,kind`’

  Insert (‘`Z2`’) or remove (‘`z2`’) a write watchpoint at addr. The number of bytes to watch is specified by kind.

  Reply:

  ‘`OK`’

    success

‘`z3,addr,kind`’ ¶
‘`Z3,addr,kind`’

  Insert (‘`Z3`’) or remove (‘`z3`’) a read watchpoint at addr. The number of bytes to watch is specified by kind.

  Reply:

  ‘`OK`’

    success

‘`z4,addr,kind`’ ¶
‘`Z4,addr,kind`’

  Insert (‘`Z4`’) or remove (‘`z4`’) an access watchpoint at addr. The number of bytes to watch is specified by kind.

  Reply:

  ‘`OK`’

    success

Next: Stop Reply Packets, Previous: Standard Replies, Up: GDB Remote Serial Protocol [Contents][Index]