#### G.5.6 MicroBlaze Features ¶

The ‘`org.gnu.gdb.microblaze.core`’ feature is required for MicroBlaze targets. It should contain registers ‘`r0`’ through ‘`r31`’, ‘`rpc`’, ‘`rmsr`’, ‘`rear`’, ‘`resr`’, ‘`rfsr`’, ‘`rbtr`’, ‘`rpvr`’, ‘`rpvr1`’ through ‘`rpvr11`’, ‘`redr`’, ‘`rpid`’, ‘`rzpr`’, ‘`rtlbx`’, ‘`rtlbsx`’, ‘`rtlblo`’, and ‘`rtlbhi`’.

The ‘`org.gnu.gdb.microblaze.stack-protect`’ feature is optional. If present, it should contain registers ‘`rshr`’ and ‘`rslr`’