#### G.5.5 LoongArch Features ¶

The ‘`org.gnu.gdb.loongarch.base`’ feature is required for LoongArch targets. It should contain the registers ‘`r0`’ through ‘`r31`’, ‘`pc`’, and ‘`badv`’. Either the architectural names (‘`r0`’, ‘`r1`’, etc) can be used, or the ABI names (‘`zero`’, ‘`ra`’, etc).

The ‘`org.gnu.gdb.loongarch.fpu`’ feature is optional. If present, it should contain registers ‘`f0`’ through ‘`f31`’, ‘`fcc`’, and ‘`fcsr`’.